Material Safety Data Sheet (MSDS)
Product Name: Polishing Liquid
Company: Huzhou Qiaoyun Polishing Co., Ltd.
Address: Building 50B, No. 258 Dongbang Road, Huzhou Economic and Technological Development Zone, Zhejiang, China
Postal Code: 313011
Phone: +86-572-3518886
Fax: +86-572-3518991
1. Chemical Composition
	Component Name
	Content (%)
	 CAS No.

	Triethanolamine Lauryl Sulfate
	15%
	/

	Nonylphenol Ethoxylate
	10%
	/

	Sodium Lauryl Sulfate
	20%
	/

	Sodium Citrate
	10%
	/

	Sodium Sulfite
	3%
	/

	Deionized Water
	[bookmark: _GoBack]Balance
	/


2. Physical and Chemical Properties
Boiling Point: ≥ 98°C
Vapor Pressure (20°C): < 3000 Pa
Evaporation Rate (Butyl Acetate=1): < 1
Density: 1.060 ± 0.02 g/cm³
Water Solubility: Easily soluble
Kinematic Viscosity: 2.6 ± 0.5 mm²/s
Appearance: Light yellow viscous liquid at room temperature
Odor: Slight
3. Fire and Explosion Data
Flash Point (Closed Cup): None
Flammability: Non-flammable
Autoignition: None
Explosion Limit: None
Firefighting Measures: Not applicable
4. Stability and Reactivity
Stability: Stable
Oxidizing Properties: None
Self-Reactivity / Explosion Hazard: None
Reaction with Water: No known skin hazards
Reactivity Caution: Avoid mixing with high-concentration electrolyte solutions
5. Health Hazard Information
Primary Exposure Routes: Inhalation, skin contact
Skin Corrosiveness: None
Irritation (Skin, Eyes): Mild irritation
Allergic Reactions: No known reports
Acute Toxicity (Oral, rat): LD₅₀ ≥ 4.5 g/kg (low toxicity)
Acute Toxicity (Oral, rabbit): LD₅₀ ≥ 2.3 g/kg (low toxicity)
Subacute Toxicity: Long-term or repeated contact may cause defatting, dryness, or dermatitis
Chronic Toxicity / Carcinogenicity / Mutagenicity / Reproductive or Developmental Toxicity: No data or reports available
Other Effects: If ingested, may irritate gastric mucosa causing vomiting, stomach pain, diarrhea
6. Emergency and First Aid Measures
General: Remove the person from the exposure site immediately
Inhalation: Move to fresh air; seek medical attention; provide oxygen if breathing is difficult; administer CPR if breathing has stopped
Eye Contact: Rinse eyes with plenty of water for at least 60 seconds; seek medical attention
Skin Contact: Rinse thoroughly with water
Ingestion: Do not induce vomiting; seek immediate medical attention
7. Special Protection
Respiratory Protection: Normally not required in well-ventilated areas; NIOSH/MESA equipment necessary in confined spaces
Ventilation: Adequate ventilation required to control exposure
Gloves: Oil-resistant (e.g. neoprene or plastic)
Eye Protection: Safety glasses or goggles
Other Clothing/Equipment: Waterproof apron if splashing is possible to prevent contamination and reduce skin contact
8. Spill and Leak Procedures
Handling & Storage Precautions: Keep away from heat and flames; avoid strong shaking during handling
In Case of Spill: Stop the leak; prevent water intrusion; absorb with suitable material; avoid entry into sewers or water bodies to prevent secondary hazards
9. Waste Disposal
Dispose of waste through authorized agencies approved by local governments; illegal disposal is strictly prohibited
10. Ecological Information
Ecotoxicity: Non-toxic
Bioaccumulation Potential: No known data
11. Transport Information
Proper Shipping Name: Polishing Liquid
Hazard Class: Non-flammable liquid
Note: The above information is based on currently available data and is not a guarantee of safety under all usage, handling, or storage conditions.
12. Regulatory Information
This MSDS is aligned with the regulations stated in the Regulations on the Safety Administration of Hazardous Chemicals (China), covering production, use, storage, transportation, and handling.
13. Other Information
Date of Issue: September 2013
Prepared by: Production Department
Reviewed by: Engineering Department
Remarks: This information is prepared based on current knowledge. Please verify its applicability before use.
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